{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":75,"n_cols":8,"rows_kept":75,"flags":["formulas_cached_only"]}
["本列表依据接环系统的法兰距排列，从小到大。本列表包括静态与活动影像拍摄设备所用的镜头接环系统。"]
[]
["厂商或产品","接环名称","画幅","用途","直径","螺纹参数","固定结构","法兰距"]
[null,"D mount","8 mm","电影和闭路电视","15.88 mm","32 TPI","螺纹","12.29 mm"]
[null,"CS mount","16 mm","电影, 闭路电视,                 工业用途, 科研","25.40 mm","32 TPI","螺纹","12.52 mm"]
[null,"C mount","16 mm","电影, 闭路电视,               工业用途, 科研","25.40 mm","32 TPI","螺纹","17.526 mm"]
["索尼NEX","索尼E接环","23.4 mm × 15.6 mm APS-C","数码静态摄影                   和摄录机","46.1 mm",null,"卡口","18 mm"]
["Canon EX",null,null,"摄录机",null,null,"卡口","20 mm"]
["奥巴E-P1,松下G1, GH1, GF1","微4/3系统","17.3 mm × 12.98 mm","数码静态摄影                   和摄录机","~38 mmA[›]",null,"卡口","20 mm"]
["Bolex",null,"16 mm","电影",null,null,"闩管","23.22 mm"]
["三星NX","NX mount","23.4 mm × 15.6 mm APS-C","数码静态摄影","42 mm",null,"卡口","25.5 mm"]
["宾得Auto 110",null,"110胶片","摄影",null,null,"卡口","27 mm"]
["美能达/徕卡M卡口","M mount","35 mm","摄影和数码静态摄影","44 mm",null,"卡口","27.80 mm"]
["莱兹/美能达CL，         美能达CLE","compact M mount","35 mm","摄影","44 mm",null,"卡口","27.80 mm"]
["柯尼卡 Hexar RF","KM mount","35 mm","摄影","44 mm",null,"卡口","28 mm             (27.80 mm?)"]
["佳能螺纹口",null,"35 mm","摄影","M39","1 mm","螺纹"]
["徕卡M39螺纹口","M39","35 mm","摄影, enlargers","M39","26 TPI","螺纹","28.80 mm"]
["Narciss",null,"16 mm","摄影","M24","1 mm","螺纹","28.8 mm"]
["en:Olympus Pen F:          奥林巴斯PEN F",null,"35 mm half-frame","摄影",null,null,"卡口","28.95 mm"]
["康泰时 G",null,"35 mm","摄影",null,null,"闩管","29.00 mm"]
["哈苏 Xpan",null,"35 mm panoramic","摄影",null,null,"卡口","34.27 mm"]
["尼康旁轴相机","en:Nikon S-Mount","35 mm","摄影",null,null,"卡口","34.85 mm"]
["Alpa",null,"35 mm","摄影",null,null,"卡口","37.80 mm"]
["美能达Vectis","V mount","30.2 mm × 16.7 mm APS","摄影和数码静态摄影",null,null,"卡口","36.00 mm (38 mm?)"]
["奥林巴斯E系列单反，松下LumixDMC-L,             徕卡Digilux","4/3系统","17.3 mm × 12.98 mm","数码静态摄影","~44 mmA[›]",null,"卡口","38.67 mm"]
["en:Aaton universal",null,"16 mm","电影",null,null,"闩管","40 mm"]
["柯尼卡F卡口","Konica F mount","35 mm","摄影","40 mm",null,"卡口","40.50 mm"]
["柯尼卡AR卡口","AR mount","35 mm","摄影","47 mm",null,"卡口","40.50 mm (40.7 mm)"]
["Miranda Camera Company","M44","35 mm和APS-C","摄影, 工业用途",null,null,"卡口","41.5 mm"]
["佳能R卡口",null,"35 mm","摄影",null,null,"闩管","42 mm"]
["佳能FL卡口",null,"35 mm","摄影",null,null,"闩管","42 mm"]
["佳能FD接环镜头","FD mount","35 mm","摄影",null,null,"闩管","42.00 mm"]
["富士卡X口",null,"35 mm","摄影","49 mm",null,"卡口","43.5 mm"]
["美能达MD卡口","MD mount","35 mm","摄影, 医学",null,null,"卡口 (54°)","43.50 mm"]
["Petriflex",null,"35 mm","摄影",null,null,"闩管","43.5 mm"]
["佳能EF接环镜头","EF mount (aka ZE)","35 mm","摄影","54 mm[1]",null,"卡口","44.00 mm"]
["佳能EF-S接环镜头","EF mount","APS-C","数码静态摄影","54 mm",null,"卡口","44.00 mm"]
["适马SA卡口",null,"35 mm","摄影",null,null,"卡口","44.00 mm"]
["Paxette",null,"35 mm","摄影","M39","1 mm","螺纹","44 mm"]
["Praktica B",null,"35 mm","摄影",null,null,"卡口","44.40 mm"]
["美能达/柯尼卡美能达α单反, 索尼α单反","A mount (也叫MA)","35 mm和APS-C","摄影和数码静态摄影,          工业用途","49.7 mm",null,"卡口 (54°)","44.5 mm"]
["禄莱福莱SL35",null,"35 mm","摄影",null,null,"卡口","44.6 mm"]
["Exakta, Topcon",null,"35 mm","摄影",null,null,"卡口","44.7 mm"]
["宾得K口","K mount (也叫PK口)","35 mm","摄影",null,null,"卡口","45.50 mm"]
["Asahiflex单反                （宾得前身）",null,"35 mm","摄影","37 mm","1 mm","螺纹","45.5 mm"]
["Praktica","M42 lens mount(aka ZS)","35 mm","摄影","42 mm","1 mm","螺纹","45.50 mm"]
["雅西卡/康泰时","Y/C mount","35 mm","摄影",null,null,"卡口","45.5 mm"]
["玛米亚ZE",null,"35 mm","摄影",null,null,"卡口","45.5 mm"]
["京瓷雅西卡 230AF","MA mount","35 mm","摄影",null,null,"卡口","~45.8 mm"]
["奥林巴斯OM","OM mount","35 mm","摄影","46 mm",null,"卡口","46 mm"]
["尼康F卡口","Nikon F mount","35 mm","摄影, 工业用途","44 mm",null,"卡口","46.5 mm"]
["Leica R","R mount","35 mm","摄影",null,null,"卡口","47.00 mm"]
["en:Contax-N",null,"35 mm","摄影",null,null,"卡口","48 mm"]
["Praktina",null,"35 mm","摄影",null,null,"闩管","50 mm"]
["腾龙","T型螺纹                         （早期型号）","35 mm","摄影","M37","0.75mm","螺纹","50.2 mm"]
["en:Arri standard",null,"35 mm和16 mm","电影",null,null,"锁扣","52 mm"]
["en:Arri mount",null,"35 mm和16 mm","电影",null,null,"卡口","52 mm"]
["en:Arri PL",null,"35 mm和16 mm","电影",null,null,"闩管","52 mm"]
["腾龙","T2","35 mm","摄影, 工业用途","42 mm","0.75 mm","螺纹","55 mm"]
["Panavision en:PV mount",null,"35 mm","电影",null,null,"闩管","57.15 mm"]
["玛米亚 7/7II",null,"6×7","摄影",null,null,"卡口","60 mm (大约)"]
["Mitchell BNCR               mount",null,"35 mm","电影",null,null,"闩管","61.468 mm"]
["玛米亚645",null,"6×4.5","摄影",null,null,"卡口","63.3 mm"]
["en:Leitz Visoflex II/III",null,"35 mm","摄影",null,null,"卡口              (Leica M)","68.8 mm"]
["宾得645",null,"6×4.5","摄影",null,null,"卡口","70.87 mm"]
["en:Arri Maxi PL",null,"70 mm","电影","64 mm",null,null,"73.5 mm"]
["Pentacon Six]]",null,"6×6","摄影",null,null,"闩管","74.1 mm"]
["哈苏",null,"6×6","摄影",null,null,"卡口","74.9 mm"]
["en:Kowa Six                   /Super 66",null,"6×6","摄影",null,null,"闩管","79 mm"]
["宾得6x7",null,"6×7","摄影",null,null,"卡口","84.95 mm"]
["en:Leitz Visoflex I",null,"35 mm","摄影","M39","26 TPI","螺纹","91.3 mm"]
["en:Bronica S2A",null,"6×6","摄影","57 mm",1,"卡口","101.7 mm"]
["禄莱福莱SL66",null,"6×6","摄影",null,null,"卡口","102.8 mm"]
["玛米亚RZ67",null,"6×7","摄影",null,null,"卡口","105 mm"]
["玛米亚RB67",null,"6×7","摄影",null,null,"卡口","112 mm"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}